ManualsContents
SettingsHelp

# Types of IP-Fax destinations

Previous Next

The IP-Fax destination details that you must specify vary depending on the machine's configuration and the configuration of the network to which it is connected.

Depending on this machine's configuration, specify the IP-Fax destination as follows:

When not using a gatekeeper/SIP server

- From IP-Fax to IP-Fax

  Specify the IP address or host name of the receiving machine.

  Example: 192.168.1.10 (IP address)

  Example: IPFAX1 (host name)

- From IP-Fax to G3 fax

  Specify the G3 fax telephone number of the receiving machine.

  Example: 0312345678

When using a gatekeeper server

- From IP-Fax to IP-Fax

  Specify the alias telephone number of the receiving machine.

  Example: 0311119999 (alias telephone number)

- From IP-Fax to G3 fax

  Specify the G3 fax telephone number of the receiving machine.

  Example: 0312345678

When using a SIP server

- From IP-Fax to IP-Fax

  Specify the SIP user name of the receiving machine.

  Example: ABC (SIP user name)

- From IP-Fax to G3 fax

  Specify the G3 fax telephone number of the receiving machine.

  Example: 0312345678

- To send to a G3 fax via a gateway connected to a public telephone line, you must specify it's the receiver's machine telephone number. For example, if the receiver's fax number is "0312345678", specify "5678". To send from an IP-Fax to G3 fax without using gatekeeper or SIP server, you must register the gateway also.

- An alias telephone number is a number that is registered in the gatekeeper, and is available only in the network to which the gatekeeper is connected.

- Pay attention to the number of telephone number digits set in the gateway/IP address conversion table to avoid transmission error.

- SIP allows you to transmit and receive documents via an IPv6 network. This machine does not support H.323 over IPv6.

- Although the machine can have multiple IP addresses in an IPv6 environment, only one address can receive IP-Faxes.

- To send via IPv6, you must specify, for the receiver's IPv6 address and host name, the manually configured address for the receiver's fax.

- For reception when not using SIP server in an IPv6 environment, you must specify this machine's IPv6 address manually. This is not necessary if you are using SIP server.

- To send by IPv4 when using SIP server in a mixed IPv4/IPv6 environment, enter "v4:" at the beginning of the IP-Fax destination. Likewise, to send by IPv6 when using SIP server in a mixed IPv4/IPv6 environment, enter "v6:" at the beginning of the IP-Fax destination.

- "SIP call setup" is performed either by IPv4 or IPv6, depending on the configuration of your environment.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search