ManualsContents
SettingsHelp

# Specifications for the Main Unit (Types 3 and 4)

Previous Next

Configuration:

Desktop

Photosensitivity type:

OPC drum

Original scanning:

One-dimensional solid scanning system through CCD

Copy process:

Laser beam scanning and electro-photographic printing

Development:

Dry two-component magnetic brush development system

Fusing:

Direct Heating (DH) fusing

Resolution:

- Scanning originals: 600 dpi

- Copying: 600 dpi

Exposure glass:

Stationary original exposure type

Original reference position:

Rear left corner

Warm-up time (23 °C (73.4 °F), rated voltage):

- Type 3: 20 seconds

- Type 4: 22 seconds

Originals:

Sheet, book, three-dimensional object

Maximum original size:

- (mainly Europe and Asia)

  A3

- (mainly North America)

  11 × 17

Paper size:

- Tray 1:

  A4, 81/2 × 11, A5, B5 JIS

  The paper tray fence is fixed. If you wish to change the size of paper placed in this tray, contact your service representative.

- Tray 2:

  A3, A4, A5, B4 JIS, B5 JIS,

  11 × 17, 81/2 × 14, 81/2 × 13, 81/2 × 11, 81/4 × 14, 81/4 × 13, 8 × 13, 8 × 10, 71/4 × 101/2,

  8K, 16K, 11 × 15, 10 × 14, 41/8 × 91/2, C5 Env

- Tray 2 (custom size):

  Vertical: 182.0–297.0 mm (7.17–11.69 inches)

  Horizontal: 148.0–432.0 mm (5.83–17.00 inches)

- Bypass tray:

  A3, A4, A5, A6, B4 JIS, B5 JIS, B6 JIS,

  11 × 17, 81/2 × 14, 81/2 × 13, 81/2 × 11, 81/4 × 14, 81/4 × 13, 8 × 13, 8 × 10, 71/4 × 101/2, 51/2 × 81/2,

  41/8 × 91/2, 37/8 × 71/2, C5 Env, C6 Env, DL Env, 8K, 16K, 12 × 18, 11 × 15, 10 × 14

- Bypass tray (custom size):

  Vertical: 90.0–305.0 mm (3.55–12.00 inches)

  Horizontal: 148.0–457.2 mm (5.83–18.00 inches)

  In printer or facsimile mode, the maximum horizontal length of the custom size is 600.0 mm (23.62 inches).

- Duplex:

  A3, A4, A5, A6, B4 JIS, B5 JIS, B6 JIS,

  11 × 17, 81/2 × 14, 81/2 × 13, 81/2 × 11, 81/4 × 14, 81/4 × 13, 8 × 13, 8 × 10, 71/4 × 101/2, 51/2 × 81/2

  8K, 16K, 11 × 15, 10 × 14

- Duplex (custom size):

  Vertical: 90.0–297.0 mm (3.55–11.69 inches)

  Horizontal: 148.0–432.0 mm (5.83–17.00 inches)

Paper weight:

- Paper trays: 52–256 g/m2 (14 lb. Bond–140 lb. Index)

- Bypass: 52–300 g/m2 (14 lb. Bond–110 lb. Cover)

- Duplex: 52–169 g/m2 (14 lb. Bond–90 lb. Index)

For details about and recommendations concerning thick paper, see "Thick Paper", Paper Specifications and Adding Paper.

Non-reproduction area (Copier):

- Leading edge: 4.2 ± 1.5 mm (0.17 ± 0.06 inches)

- Trailing edge: 0.5–6.0 mm (0.02–0.24 inches) (3.0–6.0 mm (0.12–0.24 inches) in Duplex mode)

- Left and right edges: 0.5–4.0 mm (0.02–0.16 inches)

First copy/print time:

- Type 3:

  - Full Color: 5.7 seconds

  - B&W: 3.6 seconds

- Type 4:

  - Full Color: 4.8 seconds

  - B&W: 3.1 seconds

(A4, 81/2 × 11, 100% reproduction, feeding from tray 1, on the exposure glass)

Copy/print speed (Full Color / B&W):

- Type 3: 45 sheets/minute (A4, 81/2 × 11)

- Type 4: 55 sheets/minute (A4, 81/2 × 11)

Reproduction ratio:

- (mainly Europe and Asia)

  Preset reproduction ratios:

  - Enlargement: 400%, 200%, 141%, 122%, 115%

  - Full size: 100%

  - Reduction: 93%, 82%, 75%, 71%, 65%, 50%, 25%

- (mainly North America)

  Preset reproduction ratios:

  - Enlargement: 400%, 200%, 155%, 129%, 121%

  - Full size: 100%

  - Reduction: 93%, 85%, 78%, 73%, 65%, 50%, 25%

- Zoom: From 25 to 400% in increments of 1%

Maximum continuous copy run:

999 sheets

Paper capacity (80 g/m2, 20 lb. Bond):

- Tray 1, 2: 550 sheets

- Bypass tray: 100 sheets

Power requirements

- (mainly Europe and Asia)

  220–240 V, 8 A, 50/60 Hz

- (mainly North America)

  120–127 V, 12 A, 60 Hz

Power consumption:

- Models equipped with the ARDF:

  - Main unit only

    | Type 3 | Type 4
    --- | --- | ---
    Ready | 116 W 101 W | 116 W 101 W
    During printing | 778 W 794 W | 903 W 897 W
    Maximum | 1.7 kW 1,584 W | 1.7 kW 1,584 W

    The power level when the main switch is turned off and the power cord is plugged into an outlet: 1 W or less

  - Complete system

    | Type 3 | Type 4
    --- | --- | ---
    Maximum | 1.7 kW 1,584 W | 1.7 kW 1,584 W

    The complete system consists of the main unit, internal tray 2, lower paper trays, large capacity tray (LCT), bridge unit, Booklet Finisher SR3110, fax unit, two extra G3 interface units, Copy Data Security unit, Gigabit Ethernet, File format converter, and Wireless LAN board.

- Models equipped with the one-pass duplex scanning ADF:

  - Main unit only

    | Type 3 | Type 4
    --- | --- | ---
    Ready | 127 W 120 W | 127 W 120 W
    During printing | 810 W 780 W | 905 W 897 W
    Maximum | 1.7 kW 1,584 W | 1.7 kW 1,584 W

    The power level when the main switch is turned off and the power cord is plugged into an outlet :1 W or less

  - Complete system

    | Type 3 | Type 4
    --- | --- | ---
    Maximum | 1.7 kW 1,584 W | 1.7 kW 1,584 W

    The complete system consists of the main unit, internal tray 2, lower paper trays, large capacity tray (LCT), bridge unit, Booklet Finisher SR3110, fax unit, two extra G3 interface units, Copy Data Security unit, Gigabit Ethernet, File format converter, and Wireless LAN board.

Dimensions:

- Models equipped with the ARDF (W × D × H up to ARDF):

  670 × 682 × 895 mm (26.4 × 26.9 × 35.3 inches)

- Models equipped with the one-pass duplex scanning ADF (W × D × H up to one-pass duplex scanning ADF):

  670 × 682 × 930 mm (26.4 × 26.9 × 36.7 inches)

Space for main unit (W × D) (when the control panel is tilted 62 degrees):

1,065 × 734 mm (42.0 × 28.9 inches) (including the bypass tray and output trays)

Noise emission:

- Sound power level:

  - Main unit only

    | Type 3 | Type 4
    --- | --- | ---
    Stand-by | Less than 33.2 dB (A) | Less than 32.8 dB (A)
    Copying | Less than 66.2 dB (A) | Less than 68.0 dB (A)

  - Complete system

    | Type 3 | Type 4
    --- | --- | ---
    Stand-by | Less than 33.7 dB (A) | Less than 33.8 dB (A)
    Copying | Less than 72.2 dB (A) | Less than 73.3 dB (A)

- Sound pressure level:

  - Main unit only

    | Type 3 | Type 4
    --- | --- | ---
    Stand-by | Less than 21.0 dB (A) | Less than 21.5 dB (A)
    Copying | Less than 52.6 dB (A) | Less than 53.9 dB (A)

  - Complete system

    | Type 3 | Type 4
    --- | --- | ---
    Stand-by | Less than 20.0 dB (A) | Less than 20.5 dB (A)
    Copying | Less than 57.4 dB (A) | Less than 58.6 dB (A)

    - Sound power level and sound pressure level are actual values measured in accordance with ISO 7779.

    - Sound pressure level is measured from the position of the bystander.

    - The complete system consists of the main unit, lower paper trays, internal tray 2, large capacity tray (LCT), bridge unit, and Booklet Finisher SR3110.

Weight:

- Models equipped with the ARDF: approx. 130 kg (286.6 lb.)

- Models equipped with the one-pass duplex scanning ADF: approx. 133 kg (293.3 lb.)

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search