ManualsContents
SettingsHelp

# Copying onto Regular Size Paper from the Bypass Tray

Previous Next

Load the paper face down in the bypass tray.

[Bypass] is automatically selected.

Press the [] key.

Press [Paper Size].

Select the paper size.

Press [OK] twice.

Place the originals, and then press the [Start] key.

- For details about paper sizes that can be loaded in the bypass tray, see "Recommended Paper Sizes and Types", Paper Specifications and Adding Paper.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search