ManualsContents
SettingsHelp

# Fax Transmission and Reception

Previous Next

Standard:

G3

Resolution:

- Standard: 8 × 3.85 lines/mm, 200 × 100 dpi (Standard character), 8 × 7.7 lines/mm, 200 × 200 dpi (Detail character)

- Optional: 8 × 15.4 lines/mm (Fine character), 16 × 15.4 lines/mm, 400 × 400 dpi (Super Fine character)

Transmission time:

3 seconds at 28,800 bps, Standard resolution (JBIG transmission: 2 seconds)

Data compression method:

MH, MR, MMR, JBIG

Maximum original size:

Standard: A3, 11 × 17

Custom: 297 × 1,200 mm (11.7 × 47.3 inches)

Maximum scanning size:

297 × 1,200 mm (11.7 × 47.3 inches)

Print process:

Laser beam scanning and electro-photographic printing

Transmission speed:

33,600 / 31,200 / 28,800 / 26,400 / 24,000 / 21,600 / 19,200 / 16,800 / 14,400 / 12,000 / 9,600 / 7,200 / 4,800 / 2,400 bps (auto shift down system)

- For details about the optional units required for "Fine" and "Super Fine", see "Functions Requiring Optional Configurations", Getting Started.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search