ManualsContents
SettingsHelp

# Removing Jammed Paper When the Procedure Is Not Displayed on the Control Panel

Previous Next

Remove the jammed paper by following the procedures stated in the animation that appears on the screen and the sticker or sheet inside the front cover. This section describes how to remove jammed paper if the procedure is not displayed on the screen.

- If the error message "Paper Misfeed (C)" is displayed, pay attention to following:

  - When removing jammed paper, you can touch only those areas explicitly indicated in the manual.

  - Do not remove the fusing unit. Doing so will result in loss of print quality.

  - To remove paper that has not been fed into the fixing section correctly, remove the jammed paper through the underside of the fusing unit. If the jammed paper cannot be removed through the underside of the fusing unit, remove it from the top.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search