ManualsContents
SettingsHelp

# autonet

Previous Next

Use the "autonet" command to configure AutoNet parameters.

View settings

The following command displays the current AutoNet settings:

`msh> autonet`

Configuration

You can configure AutoNet settings.

`msh> autonet {on|off}`

- {on} means "active" and {off} means "inactive".

Current interface priority configuration display

`msh> autonet priority`

Interface priority configuration

`msh> autonet priority "interface_name"`

- You can give interface's AutoNet parameter priority.

- Priority settings are available when multiple interfaces are installed.

- wlan can be specified only when the IEEE 802.11 interface is installed.

Interface | Interface configured
--- | ---
ether | Ethernet interface
wlan | IEEE 802.11 interface

- If an interface is not selected, the current interface connection settings remain in effect.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search