ManualsContents
SettingsHelp

# Reducing or Enlarging Originals

Previous Next

This section describes methods of reducing or enlarging images by specifying a reproduction ratio, or a paper size.

Base Point

The base point of reduce/enlarge differs depending on how the original is scanned. When the original is placed on the exposure glass, the upper left corner will be the base point. When it is placed in the ADF, the bottom left corner will be the base point.

- Placing the original on the exposure glass

- Placing the original in the ADF

In addition to the functions described in this section, advanced reduce/enlarge copy functions are also available. For details about these functions, see Advanced Reduce/Enlarge Copying.

- The reproduction ratio is between 25 and 400%.

Related topics

Preset Reduce / Enlarge
Zoom
Auto Reduce / Enlarge
PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search