ManualsContents
SettingsHelp

# Current Machine Status

Previous Next

This section explains how you can check the machine's status and the items displayed. Depending on the options installed on the machine, some items might not be displayed.

- UNIX: Use the "stat" parameter and the "rsh", "rcp", "ftp", and "sftp" commands. "rsh" and "rcp" cannot be used in a Windows environment.

- telnet: Use the "status" command.

Messages | Description
--- | ---
Add staples (Booklet: Back) | The staple of booklet finisher (back) is exhausted.
Add staples (Booklet: Both) | The staple of booklet finisher is exhausted.
Add staples (Booklet: Front) | The staple of booklet finisher (front) is exhausted.
Adjusting... | The machine is initializing or calibrating.
Call Service Center | There is a malfunction in the machine.
Canceling Job... | The job is being reset.
Card/Counter not inserted | The machine is waiting for prepaid card or key.
Coin or amount not inserted | The machine is waiting for coin to be inserted.
Coin/Key Counter not inserted | The machine is waiting for coin or key counter.
Configuring... | Setting is being changed.
Cover Open: Bridge Unit Left | The cover of the bridge unit left is open.
Cover Open: Bridge Unit Right | The cover of the bridge unit right is open.
Cover Open: Duplex Unit | The cover of the duplex unit is open.
Cover Open: Finisher Front | The front cover of Finisher is open.
Cover Open: Finisher Upper | The upper cover of Finisher is open.
Cover Open: Front Cover | The front cover is open.
Cover Open: LCT | The cover of the large capacity tray is open.
Cover Open: Lower Right Cover | The lower right cover is open.
Cover Open: Upper Right Cover | The upper right cover is open.
Current Job Suspended | The current job is suspended.
Empty: Black Toner | The black toner cartridge is almost empty.
Empty: Cyan Toner | The cyan toner cartridge is almost empty.
Empty: Magenta Toner | The magenta toner cartridge is almost empty.
Empty: Yellow Toner | The yellow toner cartridge is almost empty.
Energy Saver Mode | The machine is in Energy Saver Mode.
Error: Ethernet Board | An Ethernet board error has occurred.
Error: HDD Board | A hard disk drive board error has occurred.
Error: Optional Font | An error has occurred in the font file of the machine.
Error: Parallel I/F Board | An error has occurred in the parallel interface.
Error: PDL | An error has occurred in the page description language.
Error: Rem. Certificate Renewal | An error has occurred in the remote server renewal.
Error: USB Interface | An error has occurred in the USB interface.
Error: Wireless Board | An error has occurred although you can access to the board to which Bluetooth interface unit is connected.
Error: Wireless Card | There is a problem with IEEE802.11a/g interface unit or Bluetooth interface unit, or they are not supported.
Full: Finisher Booklet Tray | Booklet tray of Finisher is full.
Full: Finisher Shift Tray | Shift tray of Finisher is full.
Full: Finisher Upper Tray | Finisher's upper tray is full.
Full: Hole Punch Receptacle | Punch Chip receptacle for hole punch is full.
Full: Internal Tray 1 | The internal tray 1 is full.
Full: Waste Toner | The waste toner is full.
Hex Dump Mode | It is a hex dump mode.
In Use: Finisher | Other functions is using Finisher.
In Use: Input Tray | Other functions is using the input tray.
In Use: Staple Unit | Other functions is using the staple unit.
Independent-supplier Toner | Toner that is not recommended is set.
Jobs Suspended | All jobs are suspended.
Key Card not inserted | The machine is waiting for key card to be inserted.
Key Card/Counter not inserted | The machine is waiting for key card or key counter to be inserted.
Key Counter not inserted | The machine is waiting for key counter to be left in it.
Loading Toner... | Toner is being supplied.
Low: Black Toner | The black toner cartridge is not set correctly, or toner is almost running out.
Low: Cyan Toner | The cyan toner cartridge is not set correctly, or toner is almost running out.
Low: Magenta Toner | The magenta toner cartridge is not set correctly, or toner is almost running out.
Low: Yellow Toner | The yellow toner cartridge is not set correctly, or toner is almost running out.
Malfunction: Ext. Charge Unit | There is a problem with the external charge unit.
Malfunction: Finisher | There is a problem with the finisher.
Malfunction: LCT | There is a problem with the large capacity tray.
Malfunction: Output Tray | There is a problem with the output tray.
Malfunction: Staple Unit | There is a problem with the staple unit.
Malfunction: Tray 1 | There is a problem with tray 1.
Malfunction: Tray 2 | There is a problem with tray 2.
Malfunction: Tray 3 | There is a problem with tray 3.
Malfunction: Tray 4 | There is a problem with tray 4.
Mismatch: Paper Size | Indicated paper tray does not contain paper of selected size.
Mismatch: Paper Size and Type | Indicated paper tray does not contain paper of selected size and type.
Mismatch: Paper Type | Indicated paper tray does not contain paper of selected type.
Nearly Full: Waste Toner | Waste toner bottle is nearly full.
Need more Staples | Stapler has almost run out of staples.
No Paper: Selected Tray | There is no paper in specified tray.
Not Detected: Black Toner | Black toner is not correctly set.
Not Detected: Cyan Toner | Cyan toner is not correctly set.
Not Detected: Fusing Unit | The fusing unit is not correctly set.
Not Detected: Input Tray | The paper feed tray is not correctly set.
Not Detected: LCT | Large capacity tray is not correctly set.
Not Detected: Magenta Toner | Magenta toner is not correctly set.
Not Detected: PCU (C) | The photoconductor unit (cyan) is not correctly set.
Not Detected: PCU (K) | The photoconductor unit (black) is not correctly set.
Not Detected: PCU (M) | The photoconductor unit (magenta) is not correctly set.
Not Detected: PCU (Y) | The photoconductor unit (yellow) is not correctly set.
Not Detected: Waste Toner Bottle | Waste toner bottle is not correctly set.
Not Detected: Yellow Toner | Yellow toner is not correctly set.
Offline | Machine is offline.
Paper in Duplex Unit | The paper remains in the duplex unit.
Paper in Finisher | The paper remains in Finisher.
Paper Misfeed: Duplex Unit | The paper has jammed in Duplex Unit.
Paper Misfeed: Finisher | The paper has jammed in Finisher.
Paper Misfeed: Input Tray | The paper has jammed in the input tray.
Paper Misfeed: Internal Path | The paper has jammed inside the machine.
Prepaid Card not inserted | The prepaid card is not inserted, or has insufficient credit.
Printing... | Printing is in progress.
Proxy User/Password Incorrect | The proxy user name and/or password setting is incorrect.
RC Gate Connection Error | RC Gate communication error has occurred.
Ready | The machine is ready to print.
Renewing Remote Certificate | The remote certificate is being renewed.
SD Card Authentication failed | SD card authentication failed.
Supplies Order Call failed | The supply order call has failed.
Tray Error: Chaptering | The paper feed tray specification error has occurred because chaptering as well as the normal paper use the same tray for printing.
Tray Error: Duplex Printing | Selected paper tray cannot be used for duplex printing.
Warming Up... | The machine is warming up.

- For details about UNIX commands, see UNIX Supplement.

- Check the error contents that may be printed in the configuration page.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search