ManualsContentsPreviousNext
Settings

# Auto Fax Reception Power-Up

This machine can be set to shut down automatically if no one has used it for a while. In these situations, even though the operation switch is off, the machine can still receive incoming documents as long as the main power switch is on.

- Reception is not possible if both the operation switch and main power switch are turned off.

- You can set whether documents are printed as soon as they are received (Immediate Reception) with the User Parameter (switch 14, bit 0) in the Facsimile Features menu. See “Parameter Settings”.

- You can also have fax documents received by Memory Reception (Substitute Reception) printed after the machine is turned on.

- Parameter Settings