ManualsContentsPreviousNext
Settings

# Specifications

Component | Specifications
--- | ---
Resolution | 200dpi/300dpi/400dpi/600dpi/1200dpi
Printing speed | Type 1: 45 ppm (A4)/47 ppm (81/2 × 11) Type 2, type 3: 50 ppm (A4)/52 ppm (81/2 × 11) (plain paper, 600 dpi 600 dpi) Printing speeds depend on the machine. Check which type of machine you have.
Interface | Standard: Ethernet interface (100BASE-TX/10BASE-T) USB 2.0 Option: Gigabit Ethernet interface (1000BASE-T/100BASE-TX/10BASE-T) IEEE 802.11a/b/g wireless LAN interface
Network protocol | TCP/IP(IPv4, IPv6), Bonjour, IPX/SPX
Printer language | Standard: PCL 5e/6, PDF, PostScript 3
Fonts | PCL 5e/6: 45, 13 International fonts PostScript 3: 136 fonts
Memory | 1 GB
Hard disk | 128 GB
USB Interface (Standard) | Supported Operating System: Windows XP/Vista/7, Windows Server 2003/2003 R2/2008/2008 R2, Mac OS 10.3.3 or later Transmission spec: USB 2.0 Standard Connectable Device: Devices corresponding to USB 2.0 Standard

- When resolution is 1200 dpi, printing speed may be slower.

- When using the Mac OS X operating system, use only the standard USB Interface. An optional USB interface board is not supported.

- When using the USB Interface (Standard) with Mac OS X 10.3.3 or later, USB 2.0 is supported.