ManualsContentsPreviousNext
Settings

# Environments where the machine can be used

This section explains safety precautions about environments where the machine can be used.

| Do not use flammable sprays or solvents in the vicinity of this machine. Doing so could result in fire or electric shock.

| Do not place vases, plant pots, cups, toiletries, medicines, small metal objects, or containers holding water or any other liquids, on or close to this machine. Fire or electric shock could result from spillage or if such objects or substances fall inside this machine.

| Keep the machine away from humidity and dust. Otherwise a fire or an electric shock might occur.

| Do not place the machine on an unstable or tilted surface. If it topples over, an injury might occur.

| Do not place heavy objects on the machine. Doing so can cause the machine to topple over, possibly resulting in injury.

| Make sure the room where you are using the machine is well ventilated and spacious. Good ventilation is especially important when the machine is used heavily.

| Keep the machine away from salt-bearing air and corrosive gases. Also, do not install the machine in places where chemical reactions are likely (laboratories, etc.), as doing so will cause the machine to malfunction.

| Do not obstruct the machine's vents. Doing so risks fire caused by overheated internal components.

| Machine sound levels exceeding LWAd > 63 dB (A) are not suitable for desk work environments, so place the machine in another room.

| Keep the machine in an area that is within optimum environmental conditions. Operating the machine in an environment that is outside the recommended ranges of humidity and temperature can cause an electrical fire hazard. Keep the area around the socket free of dust. Accumulated dust can become an electrical fire hazard.