| ManualsContentsPreviousNext |

# SADF Mode

In SADF mode, even when an original is placed page by page in the ADF, each page is automatically fed when placed.

1. Press [Original Settng].

2. Select [SADF], and then press [OK].

3. Place one page of an original, and then press the [Start] key.

4. When the machine instructs you to place another original, place the next page.

   The second and subsequent pages will be fed automatically without pressing the [Start] key.

- When [Batch] is displayed instead of [SADF], specify the SADF mode under Switch to Batch in User Tools. For details about Switch to Batch, see “Input / Output”.

- When the Sort, Combine or 1 Sided 2 Sided function has been set, press the [] key after all originals have been scanned.

- In SADF mode, an original must be set within a specified time after the previous original has been fed. You can adjust this time under SADF Auto Reset in User Tools. For details, see “Input / Output”.

- You cannot switch between 1-sided and 2-sided originals during copying.

- Input / Output