ManualsContentsPreviousNext
Settings

# Checking the Content of a Scanned Original (Preview Before Transmission)

The Preview Before Transmission function allows you to check the content of a scanned original before you send it.

- This function cannot be used with the following functions:

  - Immediate Transmission

  - Parallel Memory Transmission

  - On Hook Dial

  - Manual Dial

  - SEP Code Reception

  - When [Store Only] is set for [Store File]

  - Transmission of a stored file only

  - Memory File Transfer

Place the original, and then specify the scan settings you require.

Specify the “Original Orientation” setting correctly. If you do not, the top/bottom orientation of the original will not be displayed correctly in the preview.

For details about the setting, see “Setting the Original Orientation”.

Press [Preview].

Specify the destination, and then press the [Start] key.

The machine starts to scan the original. When scanning ends, a preview is displayed.

If you want to cancel a preview, press [Cancel].

Check the preview.

- Press [Zoom Out] or [Zoom In] to reduce or enlarge the preview image.

- Press [] [] [] [] to scroll the preview image.

- Press [Switch] under “Display File” to display another selected file.

- Press [Switch] under “Display Page” to change the displayed page.

Press [Send].

Transmission starts.

To cancel the transmission, press [Cancel Sending].

After transmission, the standby display appears.

- You can have the machine select Preview Before Transmission right after the power is turned on or whenever the [Clear Modes] key is pressed. For details, see “Changing the Default Functions of the Fax's Initial Display”.

- Setting the Original Orientation

- Changing the Default Functions of the Fax's Initial Display