| ManualsContentsPreviousNext |

# Using Web Image Monitor

1. Start a Web browser.

2. Enter "http://(machine's IP address or host name) /" in the address bar to access the printer whose settings you want to change.

   The top page of Web Image Monitor appears.

3. Click [Login].

   The dialog box for entering the user name and password appears.

4. Enter the user name and password, and then click [Login].

   Contact your administrator for information about the settings.

   The Web browser might be configured to auto complete login dialog boxes by retaining user names and passwords. This function reduces security. To prevent the browser retaining user names and passwords, disable the browser's auto complete function.

5. In the menu area, click [Configuration].

6. Under "Network", click [IPv4].

7. Check that [Active] is selected for [WINS] in the [Ethernet + Wireless LAN] column, and then enter the WINS server IPv4 address in [Primary WINS Server] and [Secondary WINS Server].

8. Click [OK].

9. `"Updating..."` appears. Wait for about one or two minutes, and then click [OK].

10. Quit Web Image Monitor.

- Using Web Image Monitor