| ManualsContentsPreviousNext |

# Programming/Changing a Scan Size

This section describes how to program a Scan Size.

1. Press [Facsimile Features].

2. Press [Scan Settings].

3. Press [Program / Change / Delete Scan Size].

4. Make sure that [Program / Change] is selected.

5. Select [Program Size 1] or [Program Size 2].

6. Enter a horizontal size using the number keys.

   Each time you press [mm] or [inch], the units switch between “mm” and “inch”.

   If you enter a length and press [mm] or [inch], the length is converted automatically according to the unit (fractions are rounded off). For example, when you enter [2], [2], and [0] in millimeters and change to “inch”, the length 8.7 “inch” is shown on the display. If you press [mm] again, “221 mm” is displayed.

   If you make a mistake, press [Clear], and then try again.

   To cancel a scan size, press [Cancel].

7. Select a vertical size, and then press [OK].

   The displayed vertical size differs depending on the selected unit. When [mm] is selected, [210 mm (A4)] and [216 mm (8 1/2)] are shown. When [inch] is selected, [8.3 inch (A4)] and [8.5 inch] are shown.

   To cancel a scan size, press [Cancel].

8. Press [Exit].

9. Press the [User Tools/Counter] key.

- You can use documents longer than 356 mm (14 inches) with the User Parameter (switch 14, bit 1) in the Parameter Settings. For details about Parameter Setting, see “Parameter Settings”.

- Parameter Settings