ManualsContentsPreviousNext
Settings

# Registering and Changing Keystroke Programs

This section explains how to program a new Keystroke Program or overwrite an old one.

You can register the following items in Keystroke Programs:

- Memory Transmission/Immediate Transmission, transmission type, destinations (except for folder destinations), Original Type, Resolution, Scan Size, Auto Density, Manual Density, Original Orientation, Original Settings, Select Line, SUB/SID/SEP/PWD Code entry, Send Later, Reception Notice, BCC Transmission, E-mail TX Results, Text, Standard Message, Label Insertion, Closed Network, SUB Code Transmission, SEP Code Reception, Fax Header Print, TX Status Report, Store File, File Type, Preview before transmission

- Program name

The following procedure explains using Send Later with the fax number “0123456789” as an example of how to register a program.

Make sure that the machine is in facsimile mode and the standby display is shown.

If the standby display is not shown, press the [Facsimile] key.

Make the settings you want to register in the program.

The procedure for programming differs depending on the items you want to register.

Press the [Clear Modes] key to cancel programming.

Press the number keys [0], [1], [2], [3], [4], [5], [6], [7], [8], [9], and then continue doing the Send Later setting until the standby display appears when you press [OK].

Press the [Program] key.

Press [Program].

When no programs are registered, proceed to step 5.

Select a program number in which “Not Programmed” is shown.

If you make a mistake, press [Cancel] and select a program number again.

When you change a Keystroke Program, press [Yes] after pressing the program number you want to change. If you make a mistake, press [No] and try again.

Enter the program name, and then press [OK].

The standby display appears.

If the program name is already registered, the name is displayed. To change the program name, press [], [], [Backspace], or [Delete All], and then try again.

You should register the program name.

To cancel a program, press [Cancel]. The display returns to that of step 5.

- Use the same procedure to register and change programs. In step 5, select the program number you want to change.

- For details about text entry, see “Entering Text”, About This Machine.

- The method of registering or changing programs for the copy function is different from that of the fax function.

- For the maximum values of the following items, see “Maximum Values”:

  - Number of destinations you can register into a Keystroke Program

  - Number of Keystroke Programs you can register

  - Number of characters you can enter for a program name

- Maximum Values

Related topics

Changing a program name