ManualsContentsPreviousNext
Settings

# General Settings

This section describes the user tools in the General Settings menu under Facsimile Features.

Quick Operation Key (1-3)

Frequently used functions programmed as Quick Operation keys are shown on the menu immediately after the power is turned on.

If [On] is selected, the Quick Operation keys can be programmed with the following items:

- On

  - Manual E-mail RX

  - Send Later

  - Subject

  - Text

  - Recept. Notice

  - E-mail TX Results

  - BCC Transmission

  - Std. Message

  - Fax Header Print

  - Label Insertion

  - Closed Network

  - SUB Code TX

  - SEP Code Reception

  - Print Memory Lock

  - TX File Status

  - RX File Status

  - Journal

  - Print Stored RX File

  - TX Status Report

  - Forwarding

  - Switch RX Mode

- Off

Up to three functions can be programmed to Quick Operation keys.

Functions that are highlighted have already been set.

Default for Quick Operation Key 1: [No] (not programmed)

Default for Quick Operation Key 2: [TX File Status]

Default for Quick Operation Key 3: [RX File Status]

Switch Title

Select the title to be shown on the destination list.

Default: [Title 1]

Search Destination

Select a destination list to be used in “Search Destination”.

You can select from the Address Book, or a registered LDAP Server.

To search from an LDAP server, it is necessary to register the LDAP server in [System Settings] and set [LDAP Search] to [On].

Default: [Address Book]

For details about “LDAP Search”, see “Administrator Tools”, Network and System Settings Reference.

Communication Page Count

Checks the transmission and reception, and totals on the display.

- Pages Sent:

  Total number of transmitted pages

- Pages Received:

  Total number of received pages

1. Press [Facsimile Features].

2. Press [General Settings].

3. Press [Communication Page Count].

4. After checking the display, press [Exit].

5. Press the [User Tools/Counter] key.

Adjust Sound Volume

Adjust the sound volume during On Hook Mode and Immediate Transmission.

Default: [level 2]

Box Setting

The following functions are for delivery and transfer of documents:

- Personal Box

- Information Box

- Transfer Box

For details about Box Setting, see “Box Settings”.

Box Setting: Print List

You can print a list of the currently registered Personal Boxes, Information Boxes, and Transfer Boxes.

On Hook Mode Release Time

Use this function to specify a time to cancel On Hook mode after you transmit using On Hook dialing.

Default: [3 minutes]

Delete Recent Destinations

You can delete destinations stored in “Recent Destinations”.

When you press [Delete Recent Destinations], a confirmation message appears. To delete the recent destinations, select [Delete].

- Box Settings