| ManualsContentsPreviousNext |

# When S/MIME Cannot Be Used

This section describes likely causes of and possible solutions for S/MIME-related problems.

Problem | Causes | Solutions
--- | --- | ---
If several destinations are selected for the broadcasting sequence, the data is sent over twice. | Encrypted e-mails are sent to the destinations for which S/MIME authentication is set, and plain text e-mails are sent to the destinations for which S/MIME authentication is not set. | Make sure S/MIME-authentication destinations are separate from plain text destinations. Contact your administrator. For details about destination settings.
When putting a signature on an e-mail using S/MIME, an e-mail address for "Sender" is not set for "From". | When S/MIME is applied, the administrator appears in the "From" field, and the sender appears in the "Reply-to" field. | Contact your administrator.

- Using S/MIME makes e-mail larger than when not using S/MIME.