ManualsContentsPreviousNext
Settings

# Erase Centre / Border

This function erases the center and/or all four sides of the original image.

This function has the following three types:

Erase Border

Erases the edge margin of the original image.

Erase Centre

Erases the center margin of the original image.

Erase Centre / Border

Erases both the center and edge margins of the original image.

- The relationship between the original orientation and the erased part is as follows:

  original | original
  --- | ---

  1. Erased part

  2. 2 99 mm (0.1 3.9 inches)

- The erase width is set to 10 mm (0.4 inches) as a default. You can change this setting under Edit in User Tools. For details about Edit, see “Edit”.

- The width of the erased margin varies depending on the reproduction ratio.

- Edit

Related topics

Erase Border (same width)
Erase Border (different width)
Erase Centre
Erase Centre / Border (same width)
Erase Centre / Border (different width)