ManualsContentsPreviousNext
Settings

# Changing Paper Thickness Settings

Select [Plain Paper 1] or [Plain Paper 2] depending on the type of plain paper.

If in System Settings, [Tray Paper Settings], you set “Paper Thickness” to [Plain Paper] for each tray's [Paper Type], you must then select [Maintenance], [Plain Paper Setting] and specify either [Plain Paper 1] or [Plain Paper 2], depending on the thickness of the loaded paper.

The default setting is Plain Paper 2.

- Select [Plain Paper 1] when paper weight is between 60 69 g/m2 (16 18 lb. Bond).

- Select [Plain Paper 2] when paper weight is between 70 90 g/m2 (19 24 lb. Bond).

Press the [User Tools/Counter] key.

Press [Maintenance].

Press [Plain Paper Setting].

Select the plain paper type for each tray depending on the paper to be set and press [OK].

Press [Exit].

Press [Exit].

- In System Settings, [Tray Paper Settings], for each tray's [Paper Type] you can specify “Paper Thickness”. For details about paper thickness, see “Recommended Paper Sizes and Types”.

- Recommended Paper Sizes and Types