| ManualsContentsPreviousNext |

# Checking the Storage Result (Memory Storage Report)

This report is printed after an original is stored in memory. It helps you review the contents and the destinations of stored originals.

- If you use Parallel Memory Transmission, the Memory Storage Report is not printed.

- You can turn this report on and off with the User Parameter (switch 03, bit 2) in the Facsimile Features menu.

- Even if the machine is set up not to print this report, it is still printed if an original could not be stored.

- You can select whether to include part of the original image on the report with the User Parameter (switch 04, bit 7) in the Facsimile Features menu.

- If user authentication is set, you can select whether to display a destination with the User Parameter (switch 04, bit 4) in the Facsimile Features menu.

- If user authentication is set, you can select whether to display a sender name with the User Parameter (switch 04, bit 5) in the Facsimile Features menu.

- For details about Parameter Setting, see “Parameter Settings”.

- Parameter Settings