| ManualsContentsPreviousNext |

# spoolsw

Use the "spoolsw" command to view and configure the Job Spool settings.

You can only specify diprint, trap, lpr, ipp, ftp, sftp, wsprn, and smb (TCP/IP) protocol.

View settings

The Job Spool setting appears.

`msh> spoolsw`

Job Spool setting

`msh> spoolsw spool {on|off}`

- Specify "on" to enable Job Spool, or "off" to disable it.

Resetting Job spool setting

`msh> spoolsw clearjob {on|off}`

- When the printer power is cut during job spooling, this determines whether to reprint the spooled job.

Protocol configuration

`msh> spoolsw diprint {on|off}`

`msh> spoolsw lpr {on|off}`

`msh> spoolsw ipp {on|off}`

`msh> spoolsw smb {on|off}`

`msh> spoolsw ftp {on|off}`

`msh> spoolsw sftp {on|off}`

`msh> spoolsw wsprn {on|off}`