ManualsContentsPreviousNext
Settings

# TSI Print (Transmitting Subscriber Identification Print)

You can have the sender's Own Name or Own Fax Number printed on documents that this machine receives.

Usually the sender's Fax Header is printed on received documents. When you receive an Internet Fax document, the e-mail address of the sender is printed. If the sender has not programmed their Fax Header, you will not be able to identify them. However, if you turn this function on, the sender's Own Name or Own Fax Number is printed instead so you can find out where the document came from.

- You can turn this function on or off in the User Parameter (switch 02, bit 3) in the Facsimile Features menu. See “Parameter Settings”.

- Parameter Settings