ManualsContentsPreviousNext
Settings

# Adding Staples

This section describes what to do when staples need replacing.

- Stapling failures or jams may occur if you use a staple cartridge other than that recommended.

Open the finisher cover on the right side of the machine.

Hold the lever, and then gently pull out the cartridge.

Hold both sides of the empty refill, pull up, and remove it.

Push the new refill into the cartridge until it clicks.

Hold the lever, and then push in the cartridge until it clicks.

Close the finisher cover.

- If you cannot remove the refill, there are staples remaining. Use all the staples, and do not add more.