ManualsContentsPreviousNext
Settings

# netware

Use the "netware" command to view and configure the NetWare settings such as the print server name or file server name. The following commands are available only when the NetWare is installed.

NetWare Printer Server Names

`msh> netware pname "character string"`

- Enter the NetWare print server name using up to 47 characters.

NetWare File Server Names

`msh> netware fname "character string"`

- Enter the NetWare file server name using up to 47 characters.

Encap type

`msh> netware encap {802.3|802.2|snap|ethernet2|auto}`

Remote Printer Number

`msh> netware rnum [0-254]`

- The default is 0.

Timeout

`msh> netware timeout [3-255]`

- The default is 15.

Printer server mode

`msh> netware mode pserver`

`msh> netware mode ps`

Remote printer mode

`msh> netware mode rprinter`

`msh> netware mode rp`

NDS context name

`msh> netware context "character string"`

SAP interval

`msh> netware sap_interval [0-3600]`

It can be entered between 0 and 3600 seconds.

Setting login mode for file server

`msh> netware login server`

Setting login mode for NDS tree

`msh> netware login tree`

Setting login mode for NDS tree name

`msh> netware tree "NDS tree name"`

File transfer protocol

`msh> netware trans {ipv4pri|ipxpri|ipv4|ipx}`

- If you do not specify the protocol, the current setting is displayed.

Protocol | Set Protocol
--- | ---
ipv4pri | IPv4+IPX(IPv4)
ipxpri | IPv4+IPX(IPX)
ipv4 | IPv4
ipx | IPX