ManualsContentsPreviousNext
Settings

# Folder transmission

The following table tells you the maximum values of the Scan to Folder function settings.

Values of Set Items for Scan to Folder

Item | Maximum value | Comments
--- | --- | ---
Number of path name characters on SMB | 128 alphanumeric characters |
Number of user name characters on SMB | 64 alphanumeric characters |
Number of password characters on SMB | 64 alphanumeric characters |
Number of server name characters on FTP | 64 alphanumeric characters |
Number of path name characters on FTP | 128 alphanumeric characters |
Number of user name characters on FTP | 64 alphanumeric characters |
Number of password characters on FTP | 64 alphanumeric characters |
Number of path name characters on NCP | 128 alphanumeric characters |
Number of user name characters on NCP | 64 alphanumeric characters |
Number of password characters on NCP | 64 alphanumeric characters |
Number of addresses you can specify at the same time | 50 addresses | You can specify a maximum of 50 directly entered destinations.
Sendable file size | 2,000 MB per file |