| ManualsContentsPreviousNext |

# Setting Up as a Remote Printer (NetWare 4.x, 5/5.1, 6/6.5)

Follow the procedure below to use the printer as a remote printer under NetWare 4.x, 5/ 5.1 and 6/6.5.

- To use the printer as a remote printer under NetWare 4.x, 5/5.1, 6/6.5, set it to NDS mode.

- Do not use the printer as a remote printer when Pure IP is used.

Setting up using NWadmin

1. From Windows, start NWadmin.

   For details about NWadmin, see the NetWare manuals.

2. Set up the network connection to a print queue. Select the object in which the print queue is located in the directory tree, and then click [Create] on the [Object] menu.

3. In the [Class of new object] box, click [Print Queue], and then click [OK].

4. In the [Print Queue Name] box, enter the name of the print queue.

5. In the [Print Queue Volume] box, click [Browse].

6. In the [Available objects] box, click the volume in which the print queue is created, and then click [OK].

7. Check the settings, and then click [Create].

8. Set up the network connection to a printer. Select the object in which the printer is located, and then click [Create] on the [Object] menu.

9. In the [Class of new object] box, click [Printer], and then click [OK]. For NetWare 5, click [Printer (Non NDPS)].

10. In the [Printer name] box, enter the printer name.

11. Select the [Define additional properties] check box, and then click [Create].

12. Assign print queues to the created printer. Click [Assignments], and then click [Add] in the [Assignments] area.

13. In the [Available objects] box, click the queue you created, and then click [OK].

14. Set up the network connection to a print server. Select a context specified, and then click [Create] on the [Object] menu.

15. In the [Class of new object] box, click [Print Server], and then click [OK]. For NetWare 5, click [Print Server (Non NDPS)].

16. In the [Print Server Name:] box, enter the print server name.

    Use the same print server name specified using Web Image Monitor.

17. Select the [Define additional properties] check box, and then click [Create].

18. Assign the printer to the created print server. Click [Assignments], and then click [Add] in the [Assignments] area.

19. In the [Available objects] box, click the queue you created, and then click [OK].

20. In the [Printers] area, click the printer you assigned, and then click [Printer Number].

21. Enter the printer number, and then click [OK]. Check the settings, and then click [OK].

    Use the same printer number specified as the remote printer number using Web Image Monitor.

22. Start the print server by entering the following from the console of the NetWare server.

    If the print server is in operation, quit and restart it.

    To exit

    `CAREE: unload pserver`

    To start

    `CAREE: load pserver [print server name]`

23. Enter the printer server name as the context name, and then press the [Enter] key.

24. Select the printer name on the context menu, and then press the [Enter] key.

Setting up using Web Image Monitor

1. Start Web Image Monitor.

2. Click [Login].

   A dialog box for entering the login user name and login password appears.

3. Enter the login user name and password, and then click [Login].

   For details about the login user name and password, consult your network administrator.

   The Web browser might be configured to auto complete login dialog boxes by retaining user names and passwords. This function reduces security. To prevent the browser retaining user names and passwords, disable the browser's auto complete function.

4. In the menu area, click [Configuration].

5. Under "Network", click [NetWare].

6. Confirm the settings, and then click [OK].

   Configuration is now complete. Wait several minutes before restarting Web Image Monitor.

7. Click [Logout].

8. Quit Web Image Monitor.

- If you cannot identify the printer you want to configure, check the printer name against the configuration page printed from the printer.

- If no printer names appear in the list, match the frame types of IPX/SPXs for the computer and printer. Use the [Network] dialog box of Windows to change the frame type of the computer.

- For details about Web Image Monitor, see "Using Web Image Monitor".

- Using Web Image Monitor