ManualsContentsPreviousNext
Settings

# Page Numbering

Use this function to print page numbers on your copies.

- You cannot use the bypass tray with this function.

Page number formats

There are six formats available for page numbering.

- P1,P2...

- 1/5,2/5...

- -1-,-2-...

- P.1,P.2...

- 1,2...

- 1-1,1-2...

Stamp position and original orientation

The page stamp positions differ according to the orientation in which you place the originals.

Press [Edit / Stamp].

Press [Stamp].

Press [Page Numbering].

Select the page numbering format.

You can change the stamp position, pages to be stamped, and numbering.

After making all settings, press [OK].

Press [OK].

- You can change the settings for Page Numbering under Stamp in User Tools. For details about Stamp, see “Stamp”.

- You can change the stamp position if Combine or Duplex is specified for use with this function under Duplex Back Page Stamping Position or Page Numbering in Combine in User Tools. For details about these settings, see “Stamp”.

- When Page Numbering is used with Combine, Magazine, or Booklet function, page numbers are printed as follows:

  - Per Original is selected in Page Numbering in Combine:

    With 1 Sided/2 Sided using the Combine function

    With the Magazine or Booklet function

  - Per Copy is selected in Page Numbering in Combine:

    With 1 Sided/2 Sided using the Combine function

  - If you combine this function with the Duplex (Top to Top) function and select [P1,P2...] or [1/5,2/5...], page numbers on the back are printed as follows:

    1. Front

    2. Back

- Stamp

Related topics

Changing the stamp position
Specifying the first printing page and start number (“P1,P2...”, “-1-,-2-...”, “P.1,P.2...”, “1,2...”)
Specifying the first printing page and start number (“1/5,2/5...”)
Specifying the first printing page and start number (“1-1,1-2...”)