| ManualsContentsPreviousNext |

# Programming/Changing Special Senders

This section describes how to program and change Special Senders.

1. Press [Facsimile Features].

2. Press [Reception Settings].

3. Press [Program Special Sender].

4. Check that [Program / Change] is selected.

5. Select the sender to program or change.

   To program new sender, press [Not Programmed].

6. Enter a sender name, and then press [OK].

   Enter a destination name using Own Name or Own Fax Number.

7. Press [Full Agreement] or [Partial Agreement].

8. Select the item you want to program.

   You must select only the item you want to program.

   To cancel these settings, press [Cancel]. The display returns to that of step 5.

9. Press [OK].

   A Special Sender is programmed.

   To program another sender, repeat the procedure from step 5.

10. Press [Exit].

11. Press the [User Tools/Counter] key.

- To specify Authorized Reception, see “Authorized Reception per Sender”.

- To specify Reception File Print Qty, see “Reception File Print Qty per Sender”.

- To specify Forwarding, see “Forwarding per Sender”.

- To specify print 2 sided, see “Print 2 Sided per Sender”.

- To specify Memory Lock, see “Memory Lock per Sender”.

- To specify paper tray, see “Paper Tray per Sender”.

- Authorized Reception per Sender

- Reception File Print Qty per Sender

- Forwarding per Sender

- Print 2 Sided per Sender

- Memory Lock per Sender

- Paper Tray per Sender