ManualsContentsPreviousNext
Settings

# Acceptable Original Sizes

This section describes the size and thickness limitations that apply to originals placed on the exposure glass or the ADF.

Original sizes and thickness

Where original is set | Acceptable original size | Maximum number of sheets | Paper thickness
--- | --- | --- | ---
Exposure glass | Up to A4 (210 × 297 mm), 81/2 × 11 (216 × 279 mm) | 1 sheet |
ADF, one-sided original | A5 to A4 (up to 1,200 mm long) 51/2 × 81/2 to 81/2 × 14 | 50 sheets: Less than 80 g/m2 (21 lb. Bond)*1 | 52 128 g/m2 (14 34 lb. Bond)
ADF, two-sided original | A5 to A4 (up to 356 mm long) 51/2 × 81/2 to 81/2 × 14 | 50 sheets: Less than 80 g/m2 (21 lb. Bond)*1 | 60 105 g/m2 (16 28 lb. Bond)

*1 Above specification depends on the paper type and condition

- You can use documents longer than 356 mm (14 inches) with the User Parameter (switch 14, bit 1) in the Parameter Settings. For details about Parameter Setting, see “Parameter Settings”.

- Parameter Settings