| ManualsContentsPreviousNext |

# Installing the PostScript 3 printer driver (IPP)

1. Quit all applications currently running.

2. Insert the CD-ROM into the CD-ROM drive.

   The installer starts.

3. Select an interface language, and then click [OK].

   The printer driver with the selected language will be installed. The English printer driver is installed when the following language is selected: Suomi, Magyar, Cestina, Polski, Portugues, Russian.

4. Click [PostScript 3 Printer Driver].

   Add Printer Wizard starts.

5. Click [Next >].

6. Click [Local printer attached to this computer], and then click [Next >].

7. Click [Create a new port:].

8. Click [SmartDeviceMonitor for Client 2] in [Type of port:], and then click [Next >].

9. Click [IPP].

10. In the [Printer URL] box, enter "http://(machine's IP address or host name)/printer" as the machine's address.

    If the server authentication is issued, to enable SSL (a protocol for encrypted communication), enter "https://(machine's IP address or host name)/printer" (Internet Explorer 5.01, or a higher version must be installed).

    (example IP address: 192.168.15.16)

    `http://192.168.15.16/printer`

    `https://192.168.15.16/printer`

    You can enter "http://machine's IP address or host name/ipp" as the machine's address.

11. Enter a name for identifying the machine in [IPP Port Name]. Use a name different from the one of any existing port.

    If a name is not specified here, the address entered in the [Printer URL] box becomes the IPP port name.

12. Click [Detailed Settings] to make necessary settings, and then click [OK].

    For information about the settings, see SmartDeviceMonitor for Client Help.

13. Click [OK].

14. Check that the name of the printer driver you want to install is selected, and then click [OK].

15. Change the name of the machine if you want, and then click [Next >].

    Select [Yes] to configure the machine as default.

16. Specify whether or not to share the machine, and then click [Next >].

17. Specify whether or not to print a test page, and then click [Next >].

18. Click [Finish].

    If the [Hardware Installation] message appears, click [Continue Anyway].

    The printer driver installation starts.

- To stop installation of the selected driver, click [Cancel] before installation is complete.

- A user code can be set after the printer driver installation. For information about user code, see the printer driver Help.

- Auto Run may not work with certain operating system settings. In that case, launch "Setup.exe" on the CD-ROM root directory.