| ManualsContentsPreviousNext |

# rhpp

Use the "rhpp" command to view and configure RHPP settings.

View settings

`msh> rhpp`

Changing rhpp port number

`msh> rhpp port [1024-65535]`

- The default is 59100.

Setting timeout

`msh> rhpp timeout [30-65535]`

- The default is 300 seconds.

- "RHPP" is an abbreviation of "Reliable Host Printing Protocol", which is a manufacturer-original printing protocol.