ManualsContentsPreviousNext
Settings

# slp

Use "slp" command to view and configure the SLP settings.

`msh> slp ttl "ttl_val[1-255]"`

- You can search the NetWare server using SLP in the PureIP environment of NetWare 5/5.1. Using the "slp" command, you can configure the value of TTL which can be used by SLP multicast packet.

- The default value of TTL is 1. A search is executed only within a local segment. If the router does not support multicast, the settings are not available even if the TTL value is increased.

- The acceptable TTL value is between 1 and 255.

- This command is available only when the NetWare is installed.