ManualsContentsPreviousNext
Settings

# Sample Copy

Use this function to check the copy settings before making a long copy run.

- This function can be used only when the Sort function is selected.

Select Sort and any other necessary functions, and then place the originals.

Enter the number of copy sets with the number keys.

Press the [Sample Copy] key.

One copy set is delivered as a sample.

If the sample is acceptable, press [Continue].

The number of copies made is the number specified, minus one for the proof copy.

- If you press [Suspend] after checking the results, return to step 1 to adjust the copy settings as necessary. You can change the settings. However, depending on the combination of functions, you may not be able to change some settings.