| ManualsContentsPreviousNext |

# Status Messages

This section describes the machine status messages.

Message | Status
--- | ---
`"Hex Dump Mode"` | In Hex Dump mode, the machine receives data in hexadecimal format. Turn off the main power switch after printing, and then turn it back on.
`"Job Suspended..."` | Printing was temporarily stopped by SmartDeviceMonitor for Client. You can resume printing via [My Job List] in SmartDeviceMonitor for Client, or via the Web Image Monitor. To resume printing via Web Image Monitor, check with your system administrator first.
`"Offline"` | The machine is offline. To start printing, switch the machine online by pressing [Online].
`"Please wait."` | This message might appear for a second or two while the machine is preparing, performing initial adjustments, or adding toner. Wait a while.
`"Printing..."` | The machine is printing. Wait a while.
`"Ready"` | This is the default ready message. The machine is ready for use. No action is required.
`"Resetting job..."` | The machine is resetting the print job. Wait until `"Ready"` appears on the display panel.
`"Setting change..."` | The machine is changing settings. You cannot use the control panel while this message is displayed. Wait a while.
`"Waiting for print data..."` | The machine is waiting for the next data to print. Wait a while.