ManualsContentsPreviousNext
Settings

# Messages Displayed When Changing the On-screen Language

This section describes possible solutions for the messages that appear on the control panel when changing the on-screen language.

- Before turning the main power switch off, see "Turning On/Off the Power", About This Machine.

Message | Solutions
--- | ---
"Reboot after card insert E01" | Turn off the main power switch, and then back on again. If the error occurs again, contact your sales or service representative.
"Download Error E02" "Power off on" | Turn off the main power switch, and then back on again. If the error occurs again, contact your sales or service representative.
"Download Error E03" "Power off on" | Turn off the main power switch, and then back on again. If the error occurs again, contact your sales or service representative.
"Download Error E04" "Power off on" | Turn off the main power switch, and then back on again. If the error occurs again, contact your sales or service representative.
"Download Error E05" "Power off on" | Turn off the main power switch, and then back on again. If the error occurs again, contact your sales or service representative.
"Download Error E06" "Power off on" | Contact your sales or service representative.
"Download Error" "Power off on E10" | Contact your sales or service representative.
"Download Error" "Power off on E11" | Turn off the main power switch, and then back on again. If the error occurs again, contact your sales or service representative.
"Download Error" "Power off on E12" | Contact your sales or service representative.
"Download Error" "Power off on E13" | Contact your sales or service representative.
"Download Error" "Power off on E14" | Turn off the main power switch, and then back on again. If the error occurs again, contact your sales or service representative.
"Download Error" "Power off on E15" | Turn off the main power switch, and then back on again. If the error occurs again, contact your sales or service representative.
"Download Error E19" "Power off on" | Turn off the main power switch, and then back on again. If the error occurs again, contact your sales or service representative.
"Download Error E20" "Power off on" | Turn off the main power switch, and then back on again. If the error occurs again, contact your sales or service representative.
"Download Error E21" "Power off on" | Turn off the main power switch, and then back on again. If the error occurs again, contact your sales or service representative.
"Download Error E22" | Turn off the main power switch, and then back on again. If the error occurs again, contact your sales or service representative.
"Download Error E24" "Power Off On" | Turn off the main power switch, and then back on again. If the error occurs again, contact your sales or service representative.
"Reboot After Card Insert E32" | Turn off the main power switch, and then back on again. If the error occurs again, contact your sales or service representative.
"No Valid Data E33" | The data in the SD card may be invalid. Contact your sales or service representative.
"No Valid Data E34" | The data in the SD card may be invalid. Contact your sales or service representative.
"No Valid Data E35" | The data in the SD card may be invalid. Contact your sales or service representative.
"No Valid Version E38" | The data in the SD card may be invalid. Contact your sales or service representative.
"Download Error E42" | Turn off the main power switch, and then back on again. If the error occurs again, contact your sales or service representative.
"Download Error E49" "Power Off On" | Firmware update is prohibited. Contact your administrator.
"No Valid Data E50" | The data in the SD card may be invalid. Contact your sales or service representative.