| ManualsContentsPreviousNext |

# wsmfp

Use the "wsmfp" command to view and configure the WSD (Device), WSD (Printer) and WSD (Scanner) settings.

View settings

`msh> wsmfp`

Comment settings

`msh> wsmfp comments "comment"`

- If you do not specify a comment, current setting is displayed.

Location configuration

`mah> wsmfp location "location"`

- If you do not specify a comment, current setting is displayed.

Presentation URL configuration

`msh> wsmfp url "URL"`

- Enter the URL string in the "URL".

WSD (Device) TCP port configuration

`msh> wsmfp devport "port_number"`

- The Default is 53000.

WSD (Printer) TCP port configuration

`msh> wsmfp prnport "port_number"`

- The Default is 53001.

WSD (Printer) timeout configuration

`msh> wsmfp prntimeout [30-65535]`

- The default is 900 seconds.

WSD (Scanner) TCP port configuration

`msh> wsmfp scnport "port_number"`

- The Default is 53002.

Comment initialization

`msh> wsmfp clear comments`

Location initialization

`msh> wsmfp clear location`

Presentation URL initialization

`msh> wsmfp clear url`