| ManualsContentsPreviousNext |

# web

Use the "web" command to display and configure parameters on Web Image Monitor.

View settings

`msh> web`

URL configuration

You can set URLs linked by clicking [URL] on Web Image Monitor.

`msh> web "ID" url http://"The URL or IP address you want to register"/`

Specify "1" or "2" for ID as the number corresponding to the URL. Up to two URLs can be registered and specified.

Resetting URLs registered as link destinations

`msh> web "ID" clear url`

Specify "1" or "2" for ID as the corresponding number to the URL.

Link name configuration

You can enter the name for URL that appears on Web Image Monitor.

`msh> web "ID" name "Name you want to display"`

Specify "1" or "2" for ID the corresponding number to the link name.

Resetting URL names registered as link destinations

`msh> web "ID" clear name`

Specify "1" or "2" for ID as the number corresponding to the link name.

Help URL configuration

You can set URLs linked by clicking "?" on Web Image Monitor.

`msh> web help http://"Help URL or IP address"/help/`

Resetting Help URL

`msh> web clear help`