| ManualsContentsPreviousNext |

# User Stamp

This section describes the user tools in the User Stamp menu under Stamp.

Program / Delete Stamp

You can register, change, or delete user stamps.

You can register up to four custom stamps with your favorite designs.

For details about how to program the user stamp, see “User Stamp”.

Stamp Format:1 4

Specify how each of registered user stamps 1 to 4 is printed.

- Stamp Position

  Specify where to print the user stamp.

  Default: [Top Right]

- Adjust Stamp Position

  You can adjust the position of the user stamp within the available ranges shown below.

  (mainly Europe and Asia)

  “Top Left” T/B: 4 118 mm, L/R: 4 118 mm

  “Top Center” T/B: 4 118 mm, L/R: 59 59 mm

  “Top Right” T/B: 4 118 mm, L/R: 4 118 mm

  “Center Left” T/B: 59 59 mm, L/R: 4 118 mm

  “Center” T/B: 59 59 mm, L/R: 59 59 mm

  “Center Right” T/B: 59 59 mm, L/R: 4 118 mm

  “Bottom Left” T/B: 4 118 mm, L/R: 4 118 mm

  “Bottom Center” T/B: 4 118 mm, L/R: 59 59 mm

  “Bottom Right” T/B: 4 118 mm, L/R: 4 118 mm

  (mainly North America)

  “Top Left” T/B: 0.1 4.6 inches, L/R: 0.1 4.6 inches

  “Top Center” T/B: 0.1 4.6 inches, L/R: 2.3 2.3 inches

  “Top Right” T/B: 0.1 4.6 inches, L/R: 0.1 4.6 inches

  “Center Left” T/B: 2.3 2.3 inches, L/R: 0.1 4.6 inches

  “Center” T/B: 2.3 2.3 inches, L/R: 2.3 2.3 inches

  “Center Right” T/B: 2.3 2.3 inches, L/R: 0.1 4.6 inches

  “Bottom Left” T/B: 0.1 4.6 inches, L/R: 0.1 4.6 inches

  “Bottom Center” T/B: 0.1 4.6 inches, L/R: 2.3 2.3 inches

  “Bottom Right” T/B: 0.1 4.6 inches, L/R: 0.1 4.6 inches

- Page to Stamp

  Sets whether to print the stamp on all pages or only the first page.

  Default: [All Pages]

- User Stamp