ManualsContentsPreviousNext
Settings

# Locating the NCP folder manually

This section describes how to locate the NCP folder manually.

Press [Change] under "Path".

Enter the path where the folder is located.

Press [OK].

Press [Connection Test] to check the path is set correctly.

Press [Exit].

- If you set "Connection Type" to [NDS], and if the NDS tree name is "tree", the name of the context including the volume is "context", the volume name is "volume" and the folder name is "folder", then the path will be "\\tree\volume\context\folder".

- If you set "Connection Type" to [Bindery], and if the NetWare server name is "server", the volume name is "volume" and the folder name is "folder", then the path will be "\\server\volume\folder".

- You can enter a path using up to 128 characters.

- If the connection test fails, check the settings, and then try again.