ManualsContents
SettingsHelp

# Using telnet

Previous Next

Follow the procedure below to use telnet.

- Only one user at a time can log in to perform remote maintenance.

- If you are using Windows Vista/7, you must enable the telnet server and telnet client beforehand.

Use the IP address or the host name of the machine to start telnet.

`% telnet "IP address"`

For example, if the machine's IP address is "192.168.15.16", enter the address as follows:

`% telnet 192.168.15.16`

Enter your user name and password.

For details about the user name and password, consult your network administrator.

Enter a command.

Quit telnet.

`msh> logout`

A message asking you to confirm saving the changes appears.

Enter "yes" to save the changes, and then press the [Enter] key.

If you do not want to save the changes, enter "no", and then press the [Enter] key. To make further changes, enter "return" at the command line, and then press the [Enter] key.

- If the message "Can not write NVRAM information" appears, the changes are not saved. Repeat the procedure above.

- When the changes are saved, the network interface board is reset automatically with that changes.

- When the network interface board resets, the print job in print process will be printed. However, print jobs in queue will be canceled.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search