ManualsContents
SettingsHelp

# web

Previous Next

Use the "web" command to display and configure parameters on Web Image Monitor.

View settings

`msh> web`

URL configuration

You can set URLs linked by clicking [URL] on Web Image Monitor.

`msh> web "ID" url http://"The URL or IP address you want to register"/`

Specify "1" or "2" for ID as the number corresponding to the URL. Up to two URLs can be registered and specified.

Resetting URLs registered as link destinations

`msh> web "ID" clear url`

Specify "1" or "2" for ID as the corresponding number to the URL.

Link name configuration

You can enter the name for URL that appears on Web Image Monitor.

`msh> web "ID" name "Name you want to display"`

Specify "1" or "2" for ID as the number corresponding to the link name.

Resetting URL names registered as link destinations

`msh> web "ID" clear name`

Specify "1" or "2" for ID as the number corresponding to the link name.

Help URL configuration

You can set URLs linked by clicking "?" on Web Image Monitor.

`msh> web help http://"Help URL or IP address"/help/`

Resetting Help URL

`msh> web clear help`

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search