ManualsContents
SettingsHelp

# Unauthorized Copy Preventn.

Previous Next

Unauthorized Copy Prevention Setting

Select whether or not to specify unauthorized copy prevention on the machine.

Default: [Off]

Setting Priority (Drvr/Cmnd/Mach)

Select the unauthorized copy prevention setting on which to prioritize.

- Driver / Command

  Prints documents using the settings specified in the printer driver or commands.

- Driver/Command (Most Settgs)

  Prints the background pattern, color, and density as specified on the machine. For other items, the settings configured in the printer driver or commands are applied when printing.

- Machine Setting(s)

  Prints documents using the settings specified on the machine regardless of the printer driver settings.

Default: [Driver / Command]

Unauthorized Copy Prevention Type

Select the Unauthorized Copy Prevention type to use.

- Data Secrty. for Copying

  If the printed document is copied, scanned, or stored in the Document Server using a copier or MFP that has the optional Copy Data Security unit installed, images in the document are covered with gray overprint.

- Unathd. Copy Prev.: Patn.

  Embeds texts and background images for Unathd. Copy Prev.: Patn. on the printed document. When the printed document is copied, scanned, or stored in the Document Server, a text pattern appears on the background of the document to prevent illegal copying.

Default: [Unathd. Copy Prev.: Patn.]

Mask Type for Patrn./Density/Effect

Configure the background pattern, density, and effect you want to use.

- Mask Type for Pattern

  Select the pattern to be embedded in the background of the printed documents. The available options are as follows:

  None, Type 1, Type 2, Type 3, Type 4, Type 5, Type 6, Type 7, Type 8, Type 9, Type 10

  Default: [None]

- Pattern Density

  Select the density of the background pattern.

  Default: "3"

- Data Secrty. for Copying Effect

  Select the effect of data security for copying that will be applied to the copied or printed document.

  - Text and Background

  - Background Only

  Default: [Text and Background]

- Prevention Patterns Effect

  Select the effect of unauthorized copy prevention for pattern that will be applied to the copied or printed document.

  - Text and Background

  - Reverse Patterns (Text/Background)

  - Background Only

  - Text Only

  Default: [Text and Background]

Prevention Text Settings

To prevent unauthorized copying, configure settings by specifying line spacing, text positions, or other items.

- Text Selection

  Enter the text to be embedded on the printed documents to prevent unauthorized copying. The available options are as follows:

  Do not Specify, Unauthorized Copy, Illegal Copy, Void, Do not copy, Copy Restricted, Copy Prohibited, Controlled Document, Confidential Document, In Confidence, In Strictest Confidence, Confidential, PC Login User Name, File Name, Date & Time, PC Login User Name + File Name, PC Login User Name + Date & Time, File Name + Date & Time, PC Logn UserName+FileName+Date&Time, User Text 1, User Text 2

  Default: [Unauthorized Copy]

- Program/Change User Text

  Register any text that you want to be embedded for unauthorized copy prevention. Once registered, the text you want to use can be selected from [Text Selection].

- PCL Fonts for Texts

  Specify the font type to be used for the copy prevention text when using the PCL.

  Default: [Arial]

- PS Fonts for Texts

  Specify the font type to be used for the copy prevention text when using PostScript 3.

  Default: [Arial]

- Point Size

  Specify the font size of the copy prevention text by entering a value between 50 and 300 points using the number keys.

  Default: "70" points

- Carriage Return Space

  Specify the spacing of the lines between text by entering a value from 50 to 300 points using the number keys. This setting is displayed if a value other than [Off] is specified for [Repeat Text].

  Default: "70" points

- Text Angle

  Specify the rotation angle of the text. When a larger number is specified, the text is rotated counter-clock wise around the middle of the text string. Specify an angle between 0 to 359 degrees using the number keys.

  Default: "30" degree(s)

- Text Position

  Select the position where the text is inserted. This setting is displayed if 0 degrees is specified as the value for [Text Angle] and [Off] is specified as the value for [Repeat Text]. The available options are as follows:

  Top Left, Top Centre, Top Right, Center, Bottom Left, Bottom Center, Bottom Right

  Default: [Center]

- Repeat Text

  The text is printed repeatedly and down the page beginning the upper left corner of the page.

  - On

  - On: Rot 180deg on Ret

  - Off

  Default: [Off]

- For details about how to change the Printer Features, see "Accessing User Tools", Connecting the Machine/ System Settings.

- Unauthorized copy prevention can be specified in Web Image Monitor and in the printer driver. For details about how to configure the settings, see Printing Documents that are not Allowed to Duplicate.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search