ManualsContents
SettingsHelp

# ipp

Previous Next

Use the "ipp" command to view and configure the IPP settings.

View settings

The following command displays the current IPP settings:

`msh> ipp`

IPP timeout configuration

Specify how many seconds the computer waits before canceling an interrupted print job. The time can be entered between 30 and 65535 seconds.

`msh> ipp timeout [30-65535]`

IPP user authorization configuration

Use IPP user authorization to restrict users to print with IPP. The default is "off".

`msh> ipp auth {off|digest|basic}`

- User authorization settings are "basic" and "digest".

- If user authorization is specified, register a user name. You can register up to 10 users.

IPP user name configuration

Configure IPP users according to the following messages:

`msh> ipp user`

The following message appears:

`Input user number (1 to 10):`

Enter the number, user name, and password.

`IPP user name:user1`

`IPP password :*******`

After configuring the settings, the following message appears:

`IPP configuration changed.`

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search