ManualsContents
SettingsHelp

# Adding a Virtual Printer

Previous Next

Log in to Web Image Monitor in administrator mode.

About logging in, see Connecting the Machine/ System Settings for details.

Click [Configuration] on the [Device Management] menu.

Under "Printer", click [Virtual Printer Settings].

Click [Add].

In "Virtual Printer Name", enter a name for the new printer, and then select the protocol in the "Protocol" list.

The following Virtual Printer protocols are available: [TCP/IP (Unspecified, Normal)], [TCP/IP (Unspecified, Priority)], [TCP/IP (RHPP)], [TCP/IP (DIPRINT)], and [NetWare].

If you select [TCP/IP (DIPRINT)], or [NetWare] in the "Protocol" list, you cannot specify a virtual printer name.

Click [OK].

Click [Logout].

Quit Web Image Monitor.

- You can add up to 50 virtual printers. After 51 virtual printers have been added, [Add] will no longer be displayed.

Related topics

Enabling the Virtual Printer
Deleting a Virtual Printer
PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search