ManualsContents
SettingsHelp

# Programming Initial Set Up of a Special Sender

Previous Next

Configure the following settings for initial setup of the special senders function:

Authorized Reception

Specify whether or not to enable Authorized Reception for special senders.

Special Reception Function

Specify whether or not to enable the functions applied to individual special senders (such as Forwarding per Sender and Memory Lock RX per Sender)

When you select "Off" for this setting, the functions applied to special senders are disabled and the settings of "Reception Settings" for all senders are enabled.

Bypass Tray Paper Size

Specify the paper size that will be used for the bypass tray.

Use this setting when you register a special sender that uses the bypass tray for "Paper Tray per Sender".

You can select the method of specifying size between "Auto Detect", "Regular Size", and "Custom Size". If you select [Auto Detect], the machine recognizes the paper size automatically.

Press [Facsimile Features].

Press [Reception Settings].

Press [Program Special Sender].

Press [Initial Set Up].

Select the function you want to program.

Configure the Authorized Reception settings when necessary.

Press [Authorized Reception], press [On] or [Off], and then press [OK].

Configure the Special Reception Function settings when necessary.

Press [Special Reception Function], press [On] or [Off], and then press [OK].

Configure the Bypass Tray Paper Size settings when necessary.

Press [Bypass Tray Paper Size], and then press [Auto Detect], [Regular Size], or [Custom Size].

- Auto Detect

  Make sure that [Auto Detect] is selected.

- Regular Size

  Press [Regular Size], and then select a size.

- Custom Size

  Press [Custom Size], enter the vertical and horizontal sizes of the paper using the number keys, and then press [].

  Specify a vertical size from 90 mm (3.6 inches) to 305 mm (12.0 inches).

  Specify a horizontal size from 148 mm (5.9 inches) to 600 mm (23.6 inches).

  Each time you press [mm] or [inch], the units switch between "mm" and "inch". If you enter a length and change the units by pressing [mm] or [inch], it is converted automatically (fractions are rounded off).

Press [OK].

Press [Exit] twice.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search