ManualsContents
SettingsHelp

# What You Can Do with the PostScript 3 Driver

Previous Next

Print on special paper

You can print on paper other than plain paper or recycled paper, such as thick paper and special paper.

Print on custom size paper

You can specify the dimensions of the paper you want to use for printing, and print on custom size paper. You can register in the printer driver the paper sizes you frequently use.

Printing multiple pages on a sheet

You can shrink and combine multiple pages, and print them on a single sheet of paper. By using this function with the duplex printing function, you can reduce paper usage.

Printing with a layout suitable for making booklets

You can print on both sides of paper using a layout suitable for making booklets. Pages are placed on the left and right half side of a single sheet of paper, or both sides of a single sheet of paper. You can also specify how pages are arranged from "Open to Right/Down" or "Open to Left/Up".

Rotating images when printing

When printing on paper that has specific orientation, you can rotate images 180 degrees. You can also flip images horizontally.

Sorting prints

When printing multiple sets of documents such as handouts for meetings, you can have prints delivered in batches of ordered sets.

Staple/Punch output paper

You can use the finisher to staple individual sets when printing multiple sets, or to make punch holes in printed paper.

Adjust the image quality when printing

You can specify various settings such as the dithering method and resolutions to adjust the appearance of the output.

- Changing the dithering pattern

  Dithering is a technique used to reproduce colors and shades that cannot be reproduced using other printing methods. It uses groups of small dots (dithering pattern) to reproduce the appearance of those colors and shades. You can adjust the characteristics of the color reproduction by changing the dithering pattern. You can select a dithering pattern suitable for the image to be printed.

- Changing the color profiling pattern

  On the display, colors are express by a combination of red, green, and blue dots. On this machine, dots of cyan (C), magenta (M), yellow (Y), and black (K), are used instead. Colors need to be converted from RGB to CMYK before being printed. You can adjust how the colors are converted from RGB to CMYK by changing the patterns used for the conversion.

- Adjusting black printing quality

  You can select whether to print black and gray areas on a page in black color only, or by a combination of CMYK. When printing black text on color background, you can select to print the text over the background color (black over print).

- Smoothing image edges

  You can apply a smoothing process to jaggy curves to convert them into smooth curves when printing.

Store documents

You can store print jobs on the hard disk of this machine, and print them later using the operating the control panel or Web Image Monitor. Functions such as test print and secure print can be applied when printing the stored documents.

By storing the normal print job automatically in the printer, you can also prevent printed jobs being abandoned in the output tray. For details about print job restrictions, see "Preventing documents from being left unattended", Print.

Printing stamps on prints

You can stamp texts on printed pages. You can enter any stamp text, or edit the preset texts.

Unauthorized Copy Prevention

Print using the Data Security for Copying or Unauthorized Copy Prevention function.

- Unauthorized Copy Prevention for Pattern

  Use this function to embed a text and background pattern in confidential documents. If an unauthorized copy of the document is made, the background pattern and text will be clearly visible. This function makes it easy to identify unauthorized copies.

- Data Security for Copying

  If a document with an embedded copy guard pattern is copied, scanned, and/or stored in a machine with the Copy Data Security Unit, the image of the page to be printed is destroyed, and the copy's color is turned completely gray.

Reducing toner consumption during printing

To reduce toner consumption, follow the settings or printing methods below:

- Enabling the toner saving mode

- Printing color images in black and white using only the black toner

- Printing color images using only the toner or toners selected from cyan, magenta, yellow, and black

- Windows: For details about how to printing documents and configure print settings, see the printer driver Help.

- Windows: For details about how to display the help content, see "Displaying the Printer Driver Help", Print.

- Macintosh: For details about how to print documents and configure print settings, see Mac OS Configuration.

- To use the Data Security for Copying function, the Copy Data Security Unit must be installed.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search