ManualsContents
SettingsHelp

# Connecting to the IEEE 1284 Interface

Previous Next

This section describes how to connect an IEEE 1284 interface cable to the IEEE 1284 interface board.

| Properly shielded and grounded cables and connectors must be used for connections to a host computer (and/or peripheral) in order to meet emission limits.

Make sure the main power switch on the machine is off.

Turn off the main power switch of the host computer.

Connect an IEEE 1284 interface cable to the IEEE 1284 port.

You might have to use a conversion adapter to connect the cable to the interface. For details about acquiring a conversion adapter, consult your sales or service representative.

Connect the other end of the cable into the interface connector on the host computer.

Before connecting the cable to the computer, check the shape of the connector. Connect the cable firmly.

Turn on the main power switch of the machine.

Turn on the host computer.

When using Windows XP/Vista/7, and Windows Server 2003/2003 R2/2008/2008 R2, a printer driver installation screen might appear when the computer is turned on. If this happens, click [Cancel] on the screen.

- This machine does not come with a IEEE 1284 interface cable. Make sure you purchase the appropriate cable for the machine (connector shape) and your computer.

- Use a five meter (197 inch) or shorter IEEE 1284 compatible cable whose performance is guaranteed on the host computer.

- For details about how to turn on the main power switch, see "Turning On the Main Power", Getting Started.

- For details about installing the printer driver, see "Installing the Printer Driver", Driver Installation Guide.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search