ManualsContents
SettingsHelp

# Sizes Difficult to Detect

Previous Next

If the original type is one of the following, the machine might not detect its size correctly and the receiver's machine might print it on paper of the wrong size. The machine may also fail to copy or print the image on an appropriate size of paper.

If the original type is one of the following, select the paper size manually:

- Originals with indexes, tags, or other projecting parts

- Transparent originals such as OHP transparencies or translucent paper

- Dark originals with a lot of text and drawings

- Originals which partially contain a solid image

- Originals which have solid images at their edges

- Originals with glossy surfaces

- Bound originals of more than 10 mm (0.4 inches) in thickness, such as books

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search