ManualsContents
SettingsHelp

# Timer Settings

Previous Next

This section describes the user tools in the Timer Settings menu under System Settings.

Sleep Mode Timer

After a specified period has passed, or the [Energy Saver] key is pressed, the machine enters Sleep Mode in order to conserve energy.

Specify the time to elapse before Sleep Mode.

You can specify this setting only if [Sleep Mode] is set to [Enable] in [Administrator Tools] in [System Settings].

Default:

(mainly Europe and Asia)

[1 minute(s)]

The time can be set from 1 to 240 minutes, using the number keys.

(mainly North America)

[1 minute(s)]

The time can be set from 1 to 60 minutes, using the number keys.

Sleep Mode Timer may not work when error messages appear.

Depending on which Embedded Software Architecture application is installed on it, the machine might take longer than indicated to enter Sleep Mode.

Low Power Mode Timer

Set the amount of time the machine waits before switching to lower-power mode after copying has finished or the last operation is performed.

Default:

(mainly Europe and Asia)

[Off], [1 minute(s)]

The time can be set from 1 to 240 minutes, using the number keys.

(mainly North America)

[Off], [1 minute(s)]

The time can be set from 1 to 30 minutes, using the number keys.

Low Power Mode Timer may not work when error messages appear.

System Auto Reset Timer

The System Reset setting automatically switches the screen to that of the function set in Function Priority when no operations are in progress, or when an interrupted job is cleared. This setting determines the system reset interval.

The time can be set from 10 to 999 seconds, using the number keys.

Default: [On], [60 second(s)]

Copier / Document Server Auto Reset Timer (copier/Document Server)

Specifies the time to elapse before copier and Document Server modes are reset.

If [Off] is selected, the machine does not automatically switch to the user code entry screen.

The time can be set from 10 to 999 seconds, using the number keys.

Default: [On], [60 second(s)]

Facsimile Auto Reset Timer (facsimile)

Specify the time to elapse before the facsimile mode is reset.

The time can be set from 30 to 999 seconds, using the number keys.

Default: [30 second(s)]

Printer Auto Reset Timer (printer)

Specify the time to elapse before the printer function is reset.

The time can be set from 10 to 999 seconds, using the number keys.

Default: [On], [60 second(s)]

Scanner Auto Reset Timer (scanner)

Specify the time to elapse before the scanner function is reset.

If [Off] is selected, the machine will not automatically switch to the user code entry screen.

The time can be set from 10 to 999 seconds, using the number keys.

Default: [On], [60 second(s)]

Set Date

Set the date for the copier's internal clock using the number keys.

To change between year, month, and day, press [] and [].

Set Time

Set the time for the copier's internal clock using the number keys.

To change between hours, minutes and seconds, press [] and [].

(mainly Europe and Asia)

Enter the time using the 24-hour format (in 1 second increments).

(mainly North America)

Enter the time using the 12-hour format (in 1 second increments).

Auto Logout Timer

Specify whether or not to automatically log out a user when the user does not operate the machine for a specified period of time after logging in.

The time can be set from 60 to 999 seconds in one second increments, using the number keys.

Default: [On], [180 second(s)]

Weekly Timer Code

In order to make this setting, administrator authentication must be enabled. For details, see Security Guide.

If the Weekly Timer setting is enabled, you can set a password (using up to eight digits) for when the machine recovers from Off mode or Sleep mode. After the password has been registered, the screen requiring the password is displayed when you press the [Energy Saver] key or [Check Status] key during Off mode or Sleep mode. The machine will recover from Off mode or Sleep mode when you press the [Energy Saver] key or [Check Status] key after entering the password. If you select [Off], you do not have to enter a password to recover the machine from Off mode or Sleep mode.

Default: [Off]

Weekly Timer

Specify the time when the machine switches to and from Off mode or Sleep mode. This timer can be set for Monday through Sunday.

(mainly Europe and Asia)

Enter the time in [Power On Time] and [Power Off Time] using the 24-hour format.

(mainly North America)

Enter the time in [Power On Time] and [Power Off Time] using the 12-hour format.

- For details on how to access System Settings, see Accessing User Tools.

PreviousNext

1. 1. Searching by What You Want to Do
   - I Want to Save Paper
   - I Want to Convert Documents to Electronic Formats Easily
   - I Want to Register Destinations
   - I Want to Operate the Machine More Effectively
2. 2. What You Can Do with This Machine
   - You Can Customize the [Home] Screen as You Like
   - You Can Make Copies Using Various Functions
   - You Can Print Data Using Various Functions
   - You Can Utilize Stored Documents
   - You Can Send and Receive Faxes without Paper
   - You Can Send and Receive Faxes Using the Internet
   - You Can Send and Receive Faxes by Using the Machine without Fax Unit Installed
   - You Can Use the Facsimile and the Scanner in a Network Environment
   - You Can Prevent Information Leakage (Security Functions)
   - You Can Monitor and Set the Machine Using a Computer
   - You Can Prevent an Unauthorized Copy

Easy Search